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	TECHNICAL SERVICE BULLETIN
Whistle Noise At Lower Left Windshield Area - Built On Or Before 28-Apr-2022
	22-2306
01 August 2022

	

	
Model:
	Ford
2022 Bronco
	Built on or before 28-Apr-2022



Issue: Some 2022 Bronco vehicles may exhibit a whistle noise below the lower left windshield area at the bottom of the A-pillar. This may be due to a missed body sealer application at the factory. To correct this condition, follow the Service Procedure to reseal the affected body seam.
Action: Follow the Service Procedure to correct the condition on vehicles that meet all of the following criteria:
• 2022 Bronco
• Built on or before 28-Apr-2022
• Whistle noise from the lower left windshield area
Parts
	Service Part Number
	Quantity
	Description

	Obtain Locally
	As Needed
	3M® 2 Inch Wide Masking Tape Or Equivalent

	Obtain Locally
	As Needed
	Butyl - 3M® 08612 Windo Weld Round Ribbon Sealer Or Equivalent


As Needed indicates the amount of the part may vary and/or is not a whole number. Parts can be billed out as non-whole numbers, including less than 1.
Warranty Status: Eligible under provisions of New Vehicle Limited Warranty (NVLW)/Service Part Warranty (SPW)/Special Service Part (SSP)/Extended Service Plan (ESP) coverage. Limits/policies/prior approvals are not altered by a TSB. NVLW/SPW/SSP/ESP coverage limits are determined by the identified causal part and verified using the OASIS part coverage tool.
Labor Times
	Description
	Operation No.
	Time

	2022 Bronco: Install Tape, Road Test (Pass) Inspect Gap And Apply Butyl Sealer If Necessary (Do Not Use With Any Other Labor Operations)
	222306A
	1.2 Hrs.


Repair/Claim Coding
	Causal Part:
	5802012

	Condition Code:
	68



Service Procedure
1. Tape off the left side of the cowl panel and drive the vehicle above 50 mph (80 Km/h). Did taping off the cowl resolve the whistle noise? (Figure 1)
Figure 1
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(1). Yes - proceed to Step 2.
(2). No - this article does not apply. Refer to Workshop Manual (WSM), Section 100-04.
2. Remove the left A-pillar trim. Refer to WSM, Section 501-05.
3. Visually inspect for a gap in the sheet metal at the bottom of the A-pillar where it joins the rear engine compartment wall. Is a gap present? (Figure 2)
Figure 2
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(1). Yes - proceed to Step 4.
(2). No - this article does not apply.
4. Apply a liberal amount of butyl to fill the gap between the two metal panels and eliminate the air entry.
5. To assemble, reverse the removal procedure.
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