1) Remove the factory mirror.
Disconnect the electrical Connector If Equipped.
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Install the Brandmotion Mirror Torque : 17 Lb.in (1.9Nm)
2) Remove the A-pillar trim. Drivers and Passenger side.[image: Graphical user interface, application
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[image: Graphical user interface, chat or text message

Description automatically generated]
(1) 
 Loosen Bolt. Note the bolt is captured to the bracket and will not come out. Torque : 80 lb.in (9 Nm)
(2) Lift upward and outward on the side curtain airbag tether clip and position aside.
(3) Release the side curtain airbag pin-type retainer.
(4) Remove the retaining bolt for the side curtain airbag bracket to allow the air bag to be moved out of the way.
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2)Remove the Header Trim Panel
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3) Begin by routing the pin connectors of the harness up the driver A Pillar toward the mounting point for the sun visor. 
Continue feeding the 2 pin locations toward the center of the headliner.
Secure the mirror harness to the existing harness.
After connecting both harness and the mirror loosely attach the header Trim in place.
4) Route the Rear Camera harness down the passenger A-pillar to the rear cargo door.
Remove the Passenger front door scuff plate.
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Remove the Passenger front Kick Panel 
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Remove the Rear passenger Door Scuff plate panel.
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Remove the Load space scuff plate trim panel.
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Loosen the Passenger side load space trim panel at the top and back but do not remove.
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5) Remove the upper lift gate trim panel.
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6) Route the harness along the factory harness. (optionally you can remote the tape from the ends of the harness shroud and route the cable through it and retape the ends once your have the harness connected to the rear camera.)
7) Remove the spare tire.
8) Slide the camera bracket on the top two studs.
9) Temporarily place the spare tire back on the studs to check and confirm proper camera placement with respect to the spokes of the rim. 
10) One lock washer will be placed on each of the studs that the bracket is hanging on. The third lock washer will lock the nylon washer in its place on the very bottom stud. This is needed to make the wheel sit evenly on the carrier. 
11) Temporarily install the Spare Tire to verify the camera is in the correct position then remove the Spare tire
Wait to install the spare tire back on the carrier. This will give you more room to work through the steps in the next section.
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12) Feed the chassis harness connector through the marked hole, and out the rear vent of the tailgate. 
13) Place the provided strip of heat-shrink on the camera harness, then connect the camera to the harness via the top hole in the tire carrier. 
14) Turn the vehicle on and check the rear vision video connection.
15) Use a heat gun or a lighter to seal the heat shrink. Heat shrink should overlap both sides of the connections.






16) Reinstall the spare tire.
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18) Attach the mirror harness to the fuse panel using the supplied add a fuse connectors.
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19)  Power on the vehicle to test the mirror and camera.
20) Reinstall all removed panels.
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Remove the sun visor.
1. Position the sun visor screw cover aside
2. Remove the sun visor screw.
3. Release the sun visor from the roof.
4. If equipped
Disconnect the sun visor electrical connector.
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em: ind the instrument panel grab handle
Torque - 42 Ib.in (4.8 Nm)
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‘Remove the A-pillar trim panel.
1. Release the clips and the upper tab
Use the General Equipment- Iterior Trim Remover
2. Lift upward and outward on the A-pillar tim panel and disconnect the lower tabs
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Remove the sun visor clips.
1. Open the sun visor clip screw cover.
Use the General Equipment: Pick Hook
2. Remove the sun visor clip screw
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Release the clips and remove the windshield header trim panel.
Use the General Equipment: Interior Trim Remover
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Release the clips and rotate the lower steering column trim panel downward.
« Disconnect the electrical connectors
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Remove the interior rear view mirror.
1. Loosen the set screw.
Torque - 17 Ib.in (1.9 Nm)
2. Slide the interior rear view mirror upward
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Release the tabs and the clip and position the A-pillar trim panel cover aside.
Use the General Equipment: Interior Trim Remover
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Remove the A-pillar trim panel cover
1. Remove the A-pilla trim panel cover tether clip screw.
Torgue - 28 Ib.in (3.2 Nm)
2. Release the A-pilla trim panel cover tether clip from the A-pillar trim panel cover
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Remove the screws and the upper rai front trim panel
Torgue - 28 Ib.in (3.2 Nm)
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